Task 3:

- setting up:

when we giving current 25mA, we need larger voltage, (input 5V, across laserdiode 2.1V, which are larger than we did with dc input)

- sine wave:

we got good sine wave with 600 mV amplitude and offset of 5.7 Vpp